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	Potential Hazard
	Risk level

	Awkward/sustained postures - bend, reach, lift
	

	Forceful exertions - lifting
	

	Repetitive movements
	

	Vibration
	

	Compression
	

	Sharp points/edges - sharp materials
	

	Pinch points - bin lids
	

	Materials falling - bin lids
	

	Surfaces causing falls - icy, snow in winter
	

	Moving machinery
	

	Chemicals
	

	Biological pathogens - contact with waste
	

	Electrical
	

	Extreme heat/cold
	

	Noise
	

	Combustibles/flammables
	

	Risk of falling
	

	Other
	



	Risk control devices, personal protective equipment, and other safety considerations
	Training/Reference info

	
	



What are some good general safe work practices?
1. DO ensure that prior to commencement of any excavation all underground and/or overhead lines have been identified, exposed and well-marked/flagged.
1. DO ensure that traffic near roads or busy access ways is under control.
1. DO use traffic controllers/flaggers.
1. DO set up barricades.
1. DO provide ladders in the immediate area for access/egress of trenches, excavations.
1. DO ensure that here the cut back method is not possible, provide timber shoring, trench jacks, sheet piling, cage, or other approved method.
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