Safe Work Practice Handling and Installation of Fiberglass Tanks
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	Potential Hazard
	Risk level

	Awkward/sustained postures - bend, reach, lift
	

	Forceful exertions - lifting
	

	Repetitive movements
	

	Vibration
	

	Compression
	

	Sharp points/edges - sharp materials
	

	Pinch points - bin lids
	

	Materials falling - bin lids
	

	Surfaces causing falls - icy, snow in winter
	

	Moving machinery
	

	Chemicals
	

	Biological pathogens - contact with waste
	

	Electrical
	

	Extreme heat/cold
	

	Noise
	

	Combustibles/flammables
	

	Risk of falling
	

	Other
	



	Risk control devices, personal protective equipment, and other safety considerations
	Training/Reference info

	
	



1. DO ensure barricades and warning devices are in place.
1. DO ensure cables, spreader bar, cradles, ropes and web straps are in good condition.
1. DO ensure excavations are safe to enter.
1. DO wear proper PPE (including High Visibility Vests).
1. DO be conversant with hand signals used on the work site.
1. DO ensure proper anchor points are utilized.
1. DO ensure no heavy or sharp objects are utilized as spacers.
1. DO be conversant with the ERP (Emergency Response Plan).
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