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	Potential Hazard
	Risk level

	Awkward/sustained postures - bend, reach, lift
	

	Forceful exertions - lifting
	

	Repetitive movements
	

	Vibration
	

	Compression
	

	Sharp points/edges - sharp materials
	

	Pinch points - bin lids
	

	Materials falling - bin lids
	

	Surfaces causing falls - icy, snow in winter
	

	Moving machinery
	

	Chemicals
	

	Biological pathogens - contact with waste
	

	Electrical
	

	Extreme heat/cold
	

	Noise
	

	Combustibles/flammables
	

	Risk of falling
	

	Other
	



	Risk control devices, personal protective equipment, and other safety considerations
	Training/Reference info

	
	



Follow these recommendations when using equipment with hydraulic systems:
1. Before leaving the machine, lower the hydraulic work unit to the ground and relieve hydraulic pressure by moving the control valve back and forth several times.

1. Park the machine in an area where children are unlikely to come into contact with it
.
1. To keep the machine in place during transportation, lock the cylinder stops.

1. Use cylinder stops, locks, or blocks for raised equipment or components when servicing hydraulic components or performing maintenance.

1. To reduce the risk of escaping oil, make sure all the line connections within the system are tight.

1. Use a nonvolatile cleaning solution when washing parts.

1. Keep hydraulics properly adjusted for better control of the machine.
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