Safe Work Practice Use of Man-lifts and Scissor Lifts
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	Potential Hazard
	Risk level

	Awkward/sustained postures - bend, reach, lift
	

	Forceful exertions - lifting
	

	Repetitive movements
	

	Vibration
	

	Compression
	

	Sharp points/edges - sharp materials
	

	Pinch points - bin lids
	

	Materials falling - bin lids
	

	Surfaces causing falls - icy, snow in winter
	

	Moving machinery
	

	Chemicals
	

	Biological pathogens - contact with waste
	

	Electrical
	

	Extreme heat/cold
	

	Noise
	

	Combustibles/flammables
	

	Risk of falling
	

	Other
	



	Risk control devices, personal protective equipment, and other safety considerations
	Training/Reference info

	
	



What are some good general safe work practices?
1. DO Erect warning devices
1. DO Erect barricades and warning signs
1. DO Ensure flag person is on site
1. DO ensure that a swamper is utilized and identified
1. DO ensure means of communication between operator and swamper
1. DO have fall arrest protection in place
1. DO Follow manlift/scissor lift specific make/model safe work procedures (as per manufacturer instructions)
1. DO ensure all persons utilizing manlift/scissor lift are competent to do so.
1. DO perform inspections before each use
1. DO check work area to identify any overhead obstructions. Watch for sprinkler pipes, moving doorways and other obstacles
1. DO reattach the safety chain immediately after getting onto the scissor lift
1. DO use only on level surfaces as the equipment was designed to be used. Driving into a hole or over an edge can cause the unit to tip over
1. DO maintain a safe distance from the guard rails. 
1. DO NOT stand on the guard rail or on a bucket and do not use a ladder in a scissor lift. The guard rail system is there to protect you from falling
1. DO Find out and do not exceed the weight limit the lift was designed to withstand.
1. DO NOT  use scissor lift as a material hoist or personnel elevator
1.  Limit your work to the immediate area; travelling across the job site in an elevated position is prohibited
1. DO NOT store an oxygen or fuel cylinder on a scissor lift. When welding and cutting is done, the cylinders shall remain on the floor in a secured position.
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