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	Potential Hazard
	Risk level

	Awkward/sustained postures - bend, reach, lift
	

	Forceful exertions - lifting
	

	Repetitive movements
	

	Vibration
	

	Compression
	

	Sharp points/edges - sharp materials
	

	Pinch points - bin lids
	

	Materials falling - bin lids
	

	Surfaces causing falls - icy, snow in winter
	

	Moving machinery
	

	Chemicals
	

	Biological pathogens - contact with waste
	

	Electrical
	

	Extreme heat/cold
	

	Noise
	

	Combustibles/flammables
	

	Risk of falling
	

	Other
	



	Risk control devices, personal protective equipment, and other safety considerations
	Training/Reference info

	
	



1. DO ensure barricades and warning signs are in place.
1. DO ensure all monitors are in proper working condition as per the manufacturer’s recommendations.
1. DO check power supply, backup systems and batteries where applicable.
1. DO consider wind, atmospheric conditions, and sources of gas as well as other activities that could affect the work area when placing monitors.
1. DO ensure Respiratory Protection Equipment is available and serviceable.
1. DO ensure you are trained in proper use of respiratory equipment.
1. DO check monitors on a regular basis.
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