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1. Engine Shutdown:
· Ensure the engine of the vehicle or equipment being refueled is turned off before beginning the refueling process.
2. Grounding and Bonding:
· If refueling flammable liquids, ground both the vehicle or equipment and the fuel container to prevent static electricity buildup.
3. Fuel Selection and Handling:
· Use only approved fuel types and containers suitable for the vehicle or equipment specifications.
· Handle fuel containers carefully to prevent spills, using spill containment measures if necessary.
4. Control Spill Risks:
· Use drip pans or absorbent materials to control and promptly clean up any spills that occur during refueling.
· Report spills or leaks immediately to supervisors and environmental management.
5. Monitoring:
· During refueling, continuously monitor the process to ensure proper fuel flow and to detect any leaks or abnormalities.
6. Emergency Shutdown Procedure:
· In the event of a spill, leak, or suspected equipment malfunction, immediately stop the refueling process and follow the emergency shutdown procedure.
· Notify appropriate personnel and implement spill response procedures as needed.



Post-Refueling Procedure

1. Equipment Inspection:
· Inspect the refueled vehicle or equipment for leaks, ensure all fuel caps are securely fastened, and check for signs of fuel spillage.
· Conduct a final check to verify that all equipment used for refueling is properly stored and secured.
2. Waste Disposal:
· Properly dispose of used absorbents, empty containers, or other waste materials according to environmental regulations and company procedures.
3. Documentation:
· Record refueling activities, including fuel quantities, any incidents or observations, and any corrective actions taken.
· Maintain records of refueling equipment inspections, maintenance, and training sessions conducted.
4. Training and Review:
· Provide refueling procedure training to all personnel involved in refueling operations, including refuelers and operators.
· Conduct regular reviews and audits of refueling procedures to ensure compliance with safety standards and identify opportunities for improvement.


