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	Potential Hazard
	Risk level

	Awkward/sustained postures - bend, reach, lift
	

	Forceful exertions - lifting
	

	Repetitive movements
	

	Vibration
	

	Compression
	

	Sharp points/edges - sharp materials
	

	Pinch points - bin lids
	

	Materials falling - bin lids
	

	Surfaces causing falls - icy, snow in winter
	

	Moving machinery
	

	Chemicals
	

	Biological pathogens - contact with waste
	

	Electrical
	

	Extreme heat/cold
	

	Noise
	

	Combustibles/flammables
	

	Risk of falling
	

	Other
	



	Risk control devices, personal protective equipment, and other safety considerations
	Training/Reference info

	
	



What are some good general safe work practices?
1. DO ensure the right mix of fuel is used
1. DO ensure the string is installed correctly before starting
1. DO check the fuel often
1. DO shut down equipment when refueling or servicing
1. DO follow safe job procedures regarding refueling 
1. DO ensure that string mechanism is away from you and all others before starting.
1. DO ensure string does not hit fences, trees or rocks
1. DO ensure guards and protective devices are in place
1. DO use proper PPE as per manufacturers specifications
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